{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["汇总表","数智装备","养殖及服务部分"],"not_rendered":{"defined_names":4},"read":"whole","date_system":"1900"}

{"sheet":"汇总表","index":0,"n_rows":17,"n_cols":4,"rows_kept":17,"merged":[[0,0,0,3],[11,0,11,1],[15,0,15,1],[16,0,16,1]]}
["2024 年大渡口区跳磴镇蜂窝坝村种养循环生态项目（猪舍及服务）工程量清单"]
["序号","项目名称","总价报价(元)","备注"]
["一","数智装备"]
[1,"主体结构"]
[2,"漏粪系统"]
[3,"通风系统"]
[4,"智控系统"]
[5,"饲喂系统"]
[6,"喷淋系统"]
[7,"照明系统"]
[8,"饮水系统"]
["小计"]
["二","养殖及服务"]
[1,"生产资料"]
[2,"技术服务"]
["小计"]
["汇总合计"]

{"sheet":"数智装备","index":1,"n_rows":79,"n_cols":8,"rows_kept":79,"merged":[[0,0,0,7],[78,0,78,1]]}
["数智装备工程量清单"]
["序号","项目名称","参数","单位","工程量","综合单价（元）","合价（元）","备注"]
["一","结构部份","小计"]
[1,"混凝土工厂预制桩","1.预埋板800*800*20：1个\n2.钢筋Φ12：8米\n3.地脚螺栓M20*800 强度8.8级：6个\n4.混凝土C30:0.94平方\n5.垫层C20:0.34平方\n6.链接调节钢板400*20：1个\n7.短钢柱200*200*8:300mm：1个\n","个",{"v":9,"d":"9.00"}]
[2,"无砼立柱辅佐钢板","400*20，基础安装完成后使用钢插芯做好与地面齐平固定件，防腐蚀设计年限不小于20年。具体做法详见图纸","件",{"v":9,"d":"9.00"},null,null,"基础组装"]
[3,"立柱构件01","LZ01：K160*160*4*4700，成品构件，配16mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于10年，材质要求Q235B,具体做法详见图纸；","件",{"v":3,"d":"3.00"},null,null,"主体组装"]
[4,"立柱构件02","LZ02：K160*160*4*4318，成品构件，配16mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于10年，材质要求Q235B,具体做法详见图纸；","件",{"v":3,"d":"3.00"},null,null,"主体组装"]
[5,"立柱构件03","LZ03：K160*160*4*1800，成品构件，配16mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于10年，材质要求Q235B,具体做法详见图纸；","件",{"v":0,"d":"0.00"},null,null,"主体组装"]
[6,"平层构件01","GKL01：K120*80*4*4600，成品构件，配12mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于10年，材质要求Q235B,具体做法详见图纸；","件",{"v":4,"d":"4.00"},null,null,"养殖层组装"]
[7,"平层构件02","GKL02：K200*120*5*4600，成品构件，配12mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于10年，材质要求Q235B,具体做法详见图纸；","件",{"v":2,"d":"2.00"},null,null,"养殖层组装"]
[8,"平层构件03","GL01：K100*100*4*4600，成品构件，配12mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于10年，材质要求Q235B,具体做法详见图纸；","件",{"v":4,"d":"4.00"},null,null,"养殖层组装"]
[9,"平层构件04","GL02：K120*120*4*4600，成品构件，配12mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于10年，材质要求Q235B,具体做法详见图纸；","件",{"v":2,"d":"2.00"},null,null,"养殖层组装"]
[10,"顶面构件01","WML01：K140*80*4*4800，成品构件，配12mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于10年，材质要求Q235B,具体做法详见图纸；","件",{"v":3,"d":"3.00"},null,null,"屋面层组装"]
[11,"顶面构件02","LT01：C120*60*20*3*4600，成品构件，配12mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于10年，材质要求Q235B,具体做法详见图纸；","件",{"v":8,"d":"8.00"},null,null,"屋面层组装"]
[12,"顶面构件03","XG01：K80*40*3*4600，成品构件，配12mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于10年，材质要求Q235B,具体做法详见图纸；","件",{"v":4,"d":"4.00"},null,null,"屋面层组装"]
[13,"顶面构件04","LZ02，U80*40*3*4700，成品构件，配12mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于10年，材质要求Q235B,具体做法详见图纸；","件",{"v":2,"d":"2.00"},null,null,"屋面层组装"]
[14,"顶面构件05","LT03，U80*40*3*4800，成品构件，配12mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于10年，材质要求Q235B,具体做法详见图纸；","件",{"v":0,"d":"0.00"},null,null,"屋面层组装"]
[15,"平台构件01","BL01：K100*50*3*4600，成品构件，配12mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于20年。，材质要求Q235B,具体做法详见图纸；","件",{"v":2,"d":"2.00"},null,null,"养殖层组装"]
[16,"平台构件02","XTL01：K100*50*4*800，成品构件，配12mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于20年。，材质要求Q235B,具体做法详见图纸；","件",{"v":3,"d":"3.00"},null,null,"养殖层组装"]
[17,"平台构件03","XC01：K100*50*4*1800，成品构件，配12mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于20年。，材质要求Q235B,具体做法详见图纸；","件",{"v":3,"d":"3.00"},null,null,"养殖层组装"]
[18,"平台构件04","上猪平台K100*100*2*9200，成品构件，配12mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于20年。，材质要求Q235B,具体做法详见图纸；","件",{"v":1,"d":"1.00"},null,null,"养殖层组装"]
[19,"门口加固构件","C120*60*20*2.5\n成品构件，配12mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于10年，材质要求Q235B,具体做法详见图纸；","件",{"v":2,"d":"2.00"},null,null,"收边组装"]
[20,"风机加固构件","C120*60*20*2.5成品构件，预留安装空位，整体镀锌，材质要求Q244B,具体做法详见图纸；","件",{"v":2,"d":"2.00"},null,null,"收边组装"]
[21,"坡道钢板","3mm防滑钢板，","㎡",{"v":25,"d":"25.00"},null,null,"坡道组装"]
[22,"连接件01","240*120*12，成品构件，配12mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于10年，材质要求Q235B,具体做法详见图纸；","件",{"v":1,"d":"1.00"},null,null,"钢件配件"]
[23,"连接件02","200*120*12，成品构件，配12mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于10年，材质要求Q235B,具体做法详见图纸；","件",{"v":1,"d":"1.00"},null,null,"钢件配件"]
[24,"连接件03","200*50*12，成品构件，配12mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于10年，材质要求Q235B,具体做法详见图纸；","件",{"v":1,"d":"1.00"},null,null,"钢件配件"]
[25,"连接件04","280*80*12，成品构件，配12mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于10年，材质要求Q235B,具体做法详见图纸；","件",{"v":1,"d":"1.00"},null,null,"钢件配件"]
[26,"连接件05","320*150*12，成品构件，配12mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于10年，材质要求Q235B,具体做法详见图纸；","件",{"v":1,"d":"1.00"},null,null,"钢件配件"]
[27,"连接件06","100*100*12，成品构件，配12mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于10年，材质要求Q235B,具体做法详见图纸；","件",{"v":1,"d":"1.00"},null,null,"钢件配件"]
[28,"构配件","构配件链接螺栓，成品构件，满足构造要求，具体做法详见图纸；","件",{"v":1,"d":"1.00"},null,null,"钢件配件"]
[29,"连接件08","150*150*12，成品构件，配12mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于10年，材质要求Q235B,具体做法详见图纸；","件",{"v":0,"d":"0.00"},null,null,"钢件配件"]
[30,"连接件09","6mm厚T型钢板成品构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于10年，材质要求Q235B,具体做法详见图纸；","件",{"v":0,"d":"0.00"},null,null,"钢件配件"]
[31,"连接件10","260*120*12成品构件，配12mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于10年，材质要求Q235B,具体做法详见图纸；","件",{"v":0,"d":"0.00"},null,null,"钢件配件"]
[32,"连接件11","160*50*12成品构件，配12mm厚钢板构件，预留安装空位，满足构造要求，整体镀锌平均镀层厚度不得小于85μm.防腐蚀设计年限不小于10年，材质要求Q235B,具体做法详见图纸；","件",{"v":0,"d":"0.00"},null,null,"钢件配件"]
[33,"墙面装饰板","50mm岩棉夹芯板","㎡",68.28]
[34,"屋顶装饰板","50mm岩棉夹芯板","㎡",{"v":50,"d":"50.00"}]
[35,"无框玻璃墙","中空钢化玻璃5*12A+5，中空钢化，含上下结构槽件，硅酮密封胶封边","㎡",23.92]
[36,"栏杆","钢栏杆\n1.高度：H=1200\n3.包含预埋件制作安装；\n4.材质、做法符合设计及相关技术规范要求；包括栏门的安装，","m",{"v":28,"d":"28.00"}]
[37,"成品钢质防盗门","成品钢质防盗门M1022\n1.洞口尺寸：1000*2000\n2.五金配件齐全，满足图纸设计、使用功能要求","樘",{"v":1,"d":"1.00"}]
[38,"推拉窗","1.4mm厚单层玻璃\n2.塑钢窗\n3.五金配套齐全，纱网","㎡",{"v":1,"d":"1.00"}]
["二","漏粪系统","小计"]
[1,"全漏粪复合地板","BMC复合漏粪板，1500mm*600mm*40mm，缝宽23mm,单块承重力≥400KG。","块",{"v":32,"d":"32.00"}]
[2,"半漏粪地板","BMC复合漏粪板，1500mm*600mm*40mm，缝宽23mm，单块承重力≥400KG。","块",{"v":12,"d":"12.00"}]
[3,"*漏粪斗","采用HDPE高密度聚乙烯防渗膜，厚度2mm，用料面积100平米（含损耗、现场安装、辅助材料）规格3200*4700*1000","套",{"v":8,"d":"8.00"}]
[4,"*排粪管","pvc管外径Φ200x3.5mm厚，含阀门管件，安装辅料。从漏粪斗分两路分别汇入两个软体沼气袋，管路长度暂定50米。实际长度按现场确定。","米",{"v":50,"d":"50.00"}]
[5,"*软体沼气袋","软体沼气袋，材质PVC，尺寸4*4*3.2M，容量50方。进出料管用直径110mm-300mm的PVC管预埋，具体尺寸可根据实际场地自行设计，进出口管道要伸入发酵池20cm-30cm的长度，以方便安装发酵袋。","个",{"v":1,"d":"1.00"}]
["三","通风系统","小计"]
[1,"湿帘","包含内循环系统水泵220V,100W,电缆1.0平，水管32mm，及其他辅材4.8m*1.8m*0.15m；外挂安装；带水箱；水箱内带水泵浮球阀；水帘纸含铝合金1.2mm厚外框；纸张≥143张/米;波纹高7mm；进风角度45º；降温效率≥70%；纸张110g/㎡，湿帘一体","㎡",8.64]
[2,"负压风机","220V,1100W； 51高负压风机，11kw，复合扇叶；专用风机电机；⻛ 量27500m³/h---0帕⼯况，1.1kw，洞口尺寸：洞口1460mmx1460mm，复合扇叶；专用风机电机；","套",{"v":1,"d":"1.00"}]
[3,"负压风机","220V,1100W； 51高负压风机，11kw，复合扇叶；专用风机电机；⻛ 量27500m³/h---0帕⼯况，1.1kw，洞口尺寸：洞口1460mmx1461mm，复合扇叶；专用风机电机；","套",{"v":1,"d":"1.00"}]
["四","智能控制","小计"]
[1,"AI全景摄像头","※焦距：1.7mm\n※传感器：5MP SONY 1/2.8” CMOS\n※最低照度：彩色： 0.1LUX 黑白： 0LUX\n※快门：AUTO/ 1/50（ 1/60） -1/100,000sec\n※日夜模式：自动/彩色/黑白\n宽动态：DWDR\n※降噪：3D 降噪、 2D 降噪\n信噪比：信噪比≥69dB\n※视频压缩：主码流: H.265/H.264/MJPEG\n次码流: H.265/H.264/MJPEG\n三码流: H.265/H.264\n编码格式：H.265/H.264/MJPEG\n※网络接口：1 个 RJ45 以太网接口， 10/100M 自适应\n※工作环境：温度： 30℃~60℃， 湿度： 小于 95% (无冷凝)\n※防护等级：IP65；                                                    4路高清POE网络硬盘录像机，6TB硬盘，可储存30天左右数据","件",4]
[2,"硬盘录像机","4路高清POE网络硬盘录像机，6TB硬盘，可储存30天左右数据","件",1]
[3,"AI云盒","DDR2 128MB NOR FLASH 16MBYTE 12V@1A，开通串联端口，方便集成，上传云端，云端储存年限三年，便于随时调取数据。","件",1]
[4,"8口POE交换机","※固定端口：8*10/100/1000Base-T以太网端口\n2*1000 Base-X SFP光口\n※交换容量：20Gbps\n※包转发率：15Mpps\n※MAC地址：8K\n※PoE+供电：POE款型：150W（POE:125W）\n※电源：100~240V AC\n※工作温度/存储温度：0ºC～40ºC\n※工作湿度/存储湿度：5%~95%（非冷凝）\n※外形尺寸（W×H×D）mm：280mm×170mm×43.6mm","件",1]
[5,"防水电箱","445*315*125","件",1]
[6,"监控支架","铝合金喷涂","件",4]
[7,"网线","超五类无氧铜","m",90]
[8,"PVC管",{"v":2,"d":"2.00"},"m",40]
[9,"PVC配件","管卡、直通、三通、弯头","m",1]
[10,"电源线","RVV2*2.5MM","m",10]
[11,"环境监控物联网系统","配置：\n智能环境监控网关4G*1\n无线室内温度传感器*3\n无线室内湿度传感器*1","套",1]
[12,"智能控制系统","集成式控制器，集传感器、AI监控、联动风机、湿帘，实现自动联动操作，实现手机APP操作控制，实施数据上传云端，通过后台随时调动猪场数据、风机实现定时换气功能。","项",1]
["五","饲喂系统（粥料线）","小计"]
[1,"粥料搅拌罐","1、容量1000L，201不锈钢材质,2、配备推进式搅拌叶片，粥料配比搅拌系统","套",{"v":1,"d":"1.00"}]
["六","喷淋系统","小计"]
[1,"高压防爆管及喷头、堵头","喷淋管是PE材质，管直径10mm，喷头：黄铜镀镍工艺，喷洒直径60mm左，喷孔0.5毫米，喷洒流量0.03-0.08L/min，工作压力4-12kg；喷头间隔1米布置","米",{"v":40,"d":"40.00"}]
[2,"加压泵及过滤器、消毒液、除臭液灌及系统","功率60W;220V电压，水泵转换电源","台",{"v":2,"d":"2.00"}]
["七","照明系统","小计"]
[1,"照明","LEDT8，猪舍专用产品规格:1200mm长；输入功率：18W；输入电压：185V-240V；驱动类型:IC恒流防水驱动；发光颜色：白光6500K；产品材质:亚克力面罩。","盏",{"v":3,"d":"3.00"}]
[2,"灯开关","产品名称：单开双控；额定电流：10A；输入电压：250～；规格尺寸：86*86mm；面板材质：阻燃PC；安装方式：暗装；产品颜色：白色。","个",{"v":1,"d":"1.00"}]
[3,"灯主线","规格：ZR-BV2*2.5mm²；名称：单芯硬导体阻燃电线；绝缘外套材质：聚氯乙烯；导体材质：无氧铜；额定电压450V/750V；","米",{"v":35,"d":"35.00"}]
[4,"灯分支线","规格：ZR-BV2*1.5mm²；名称：单芯硬导体阻燃电线；绝缘外套材质：聚氯乙烯；导体材质：无氧铜；额定电压450V/750V；","米",{"v":30,"d":"30.00"}]
[5,"配电电柜","电箱体元器件规格型号及技术要求\n1. 断路器\n 总断路器：32A\n风机/搅拌罐断路器：16A\n照明断路器及其他：10A\n2. 开关电源\n- 提供直流24V电源，用于直流继电器。\n3. 交换机\n 配套柜内插座，电源6A。\n4. POE交换机\n 需适配摄像头等设备供电。\n5. 接触器\n匹配负载（如风机、泵）电压（默认AC220V）。\n6. 热继电器\n- 保护范围：4~7A（运行电流约5A，启动电流约6A）。\n7. 继电器\n- 交流220V：2副转换触点，触点容量5A。\n- 直流24V：2副转换触点，触点容量5A。\n8. 柜内插座\n 卡装式，用于交换机等设备供电。\n9. 接线端子\n- 导线规格：2.5平方毫米。\n10. 指示灯及选择开关\n- 指示灯：电源指示灯、运行指示灯。\n- 转换开关：手自动切换，湿帘水泵用三档（自动/停/手动），卷帘用五档。","套",1]
["八","饮水系统","小计"]
[1,"饮水器","每套名称及数量：\n1.加厚饮水管50cm，304不锈钢，1个\n2.支顶丝管卡，304不锈钢，2个\n3.支顶丝管卡固定栓304不锈钢，6个\n4.大号不锈钢饮水碗直径17CM 304不锈钢，1个\n5.自动饮水嘴 304不锈钢，1个","套",12]
[2,"引水管","4分PVC水管","米",{"v":30,"d":"30.00"}]
["汇总",{"$nulls":5},{"$f":"G76+G70+G67+G65+G52+G48+G42+G3","v":0}]

{"sheet":"养殖及服务部分","index":2,"n_rows":22,"n_cols":10,"rows_kept":22,"merged":[[0,0,0,9],[1,2,1,3],[2,1,7,1],[2,2,2,3],[3,2,3,3],[4,2,4,3],[5,2,5,3],[6,2,6,3],[7,2,7,3],[8,1,20,1],[8,2,13,2],[14,2,15,2],[16,2,16,3],[17,2,17,3],[18,2,18,3],[19,2,19,3],[20,2,20,3],[21,2,21,3]]}
["养殖及服务工程量清单"]
["序号","类别","名称",null,"规格、频次","单位","数量","单价（元）","合计金额（元）","是否一次"]
[1,"生产资料","纯种荣昌仔猪",null,"20-25kg","头",20,null,null,"否"]
[2,null,"饲料费",null,null,"头",20,null,null,"否"]
[3,null,"疫病防控",null,"含兽药、疫苗等","头",20,null,null,"否"]
[4,null,"高压清洗消毒设备",null,null,"套",1,null,null,"是"]
[5,null,"易耗品",null,"包含防疫物资等","头",20,null,null,"否"]
[6,null,"合计"]
[7,"技术服务","定期技术指导","日常饲喂管理现场指导","每周一次","次",35,null,null,"否"]
[8,null,null,"日常消毒","每周一次，含消毒物资","次",35,null,null,"否"]
[9,null,null,"日常生物安全监督指导","每周一次","次",35,null,null,"否"]
[10,null,null,"猪只消化道呼吸道提升","技术指导及产品供应","头",20,null,null,"否"]
[11,null,null,"猪只健康度提升","技术指导及产品供应","头",20,null,null,"否"]
[12,null,null,"常见猪病诊治指导","每月平均两次","次",16,null,null,"否"]
[13,null,"检测服务","异常检测","根据异常情况及时采样送检","次",35,null,null,"否"]
[14,null,null,"常规检测","猪舍内外采样每周一次、进猪前二次，含检测试剂","次",40,null,null,"否"]
[15,null,"专家培训",null,"每月二次，仅含专家费用和差旅费，不含组织费","次",8,null,null,"是"]
[16,null,"猪苗采购配送",null,null,"次",1,null,null,"是"]
[17,null,"饲料、动保采购与配送",null,"因每次数量太少需额外收取，预计每周次","次",35]
[18,null,"协助猪只出栏销售或回收",null,null,"头",20]
[19,null,"合计"]
[20,null,"总计"]