{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":187,"n_cols":4,"rows_kept":187,"merged":[[0,0,0,3],[1,0,1,3],[2,0,2,3],[3,0,3,3],[4,0,4,3],[38,0,38,2],[96,0,103,0],[96,1,103,1],[96,3,103,3],[106,0,106,2],[107,0,129,0],[131,0,146,0],[148,0,168,0],[170,0,177,0],[178,0,178,3],[186,0,186,3]],"flags":["formulas_cached_only"]}
["     医用中轴柴油监护型救护车及车载设备参数信息收集表   报价： 万"]
["生产厂家（供应商）：                     设备品牌：                                          \n型号：                                                  机器产地："]
["单位名称：                                                                              联系人： "]
["职务：                                        联系电话：                                          电子邮箱： "]
["————————————————————密封线—————————————————————"]
[1,"工作条件","（1）适应环境：车辆应适应各种自然条件，适应户外长时期作业的需求；（2）车辆适应气温-35℃到60℃之间（自然环境）；（3）相对湿度小于等于80%。","备注"]
[2,"总体要求","能在采购单位所在地公安交通管理部门办理特种车上牌照手续。"]
[3,"基本参数"]
[3.1,"外形尺寸（mm）","长:   宽:   高："]
[3.2,"医疗舱尺寸（mm）","长:   宽:   高："]
[3.3,"轴距","轴距（mm）："]
[3.4,"发动机功率（KW）"]
[3.5,"安置及驱动方式"]
[3.6,"变速器"]
[3.7,"最大总质量（kg）"]
[3.8,"发动机排量（ ml ）"]
[3.9,"燃油种类","柴油"]
[3.1,"油箱容积（L）"]
[3.11,"油耗（L/100km）"]
[3.12,"发动机型式"]
[3.13,"排放标准","★国六"]
[3.14,"制动形式"]
[3.15,"前轮距/后轮距（mm）"]
[3.16,"整备质量（kg）"]
[3.17,"额定载客（人）","≤7人"]
[3.18,"离合器"]
[3.19,"轮胎型号"]
[3.2,"转向系统"]
[3.21,"悬架系统"]
[3.22,"空调系统"]
[3.23,"制热情况","在环境温度-20摄氏度时，启动加热系统在\n      分钟内使车内温度至少达到16摄氏度以上。"]
[3.24,"制冷要求","在环境温度40摄氏度时，使车内温度至少低于环境温度      摄氏度以上。"]
[3.25,"水温","在高温环境中（自然温度60摄氏度）和驻车状态下发动机连续工作时，其水温在     摄氏以下。"]
[3.26,"安全气囊"]
[3.27,"其他","是否有电动车窗，遥控钥匙，中控锁，后视镜，原车倒车雷达、影像。中控触摸屏尺寸   "]
[3.28,"车窗"]
[3.29,"轮骰","铝合金"]
[{"v":3.3,"d":"3.30"},"脚踏","隐藏式"]
["二、救护车改装配置要求"]
[4,"外观"]
[5,"警示系统"]
[5.1,"LED警灯","顶灯要一体嵌入式"]
[5.2,"左右爆闪警灯"]
[5.3,"警灯、警报器"]
[6,"内饰","医疗舱内饰须为ABS一体吸塑成型内饰，医疗舱全部内饰不得使用木质、玻璃钢、地毯、布面、PVC和纤维类材料。"]
[7,"驾驶舱内顶"]
[8,"材料特性"]
[9,"环保性能"]
[10,"中隔墙"]
[11,"观察窗"]
[12,"密封隔离"]
[13,"医疗器械平台"]
[null,null,"器械平台上可放置监护仪、心电图机、呼吸机、除颤仪等急救设备，安装牢固，便于医护人员的观察和操作。"]
[null,null,"平台下方有3组器械柜，配有锁扣柜门；1组开放式器械柜可放置吸引器等急救用品。"]
[14,"药品柜","药品柜位于医疗舱左侧前方，分别为3层，可放置药品盒，药品分类并具有独立存放区域，便于医护人员的取放操作。"]
[null,null,"可放置湿化瓶、呼吸机接口，便于医护人员的取放操作并有明显标识。"]
[15,"内饰顶","材料"]
[null,null,"前方装是否有液晶控制系统。"]
[null,null,"吊柜"]
[null,null,"消毒灯、手术灯、输液架、安全行车扶手、对讲系统。"]
[null,null,"顶部右侧储物盒   组。"]
[null,null,"夜间外照明灯。"]
[16,"氧气瓶柜"]
[17,"医疗舱左侧饰板"]
[null,"电源系统220V"]
[null,"电源系统12V"]
[19,"储物柜"]
[20,"地板"]
[21,"护士座椅"]
[22,"医生座椅"]
[23,"长排柜式座椅"]
[24,"扶手"]
[25,"控制系统"]
[26,"功能界面"]
[27,"电源系统"]
[28,"专用电瓶"]
[29,"逆变器"]
[30,"外接充电系统"]
[31,"安全保护"]
[32,"供氧系统"]
[33,"管道"]
[34,"氧气瓶"]
[35,"高压减压阀"]
[36,"湿化瓶"]
[37,"杀菌系统"]
[38,"照明灯"]
[39,"顶射灯"]
[40,"对讲系统"]
[41,"输液固定系统"]
[42,"通讯系统"]
[43,"其他"]
[44,"安全要求","每个座位配安全带。"]
[45,"保护措施","医疗舱内均为过渡软包装，内部表面没有尖锐的物体，所有医疗设备的挂钩、托架应紧贴舱壁安装，周围有保护措施。"]
[46,"内壁加固","医疗舱内壁加固防撞处理。"]
[47,"防撞垫","侧门上车头部防撞保护。"]
[48,"担架系统"]
[48.1,"自动上车担架","1.主要材料：","样式"]
[null,null,"2.担架垫材质，厚度XXmm，分体式：担架面支架可分离。"]
[null,null,"3.尺寸：高位时(长*宽*高) XX cm，低位时(长*宽*高)XXcm"]
[null,null,"4.靠背最大倾角："]
[null,null,"5.膝部最大倾角："]
[null,null,"6.自重："]
[null,null,"7.承重："]
[null,null,"8.轮子尺寸："]
[48.2,"担架平台","担架安装组合平台"]
[49,"其他"]
["车载设备"]
["呼\n吸\n机","一、主机部分："]
[null,"1. 是否气动气控，不需要电源和蓄电池，配备2 L氧气瓶；"]
[null,"2.是否带手动通气，用于紧急情况；"]
[null,"3.范围：是否成人、儿童；"]
[null,"4.是否背包式，方便携带。"]
[null,"5.是否气源压力低时有报警"]
[null,"二、性能参数："]
[null,"1.分钟通气量："]
[null,"2.呼吸频率："]
[null,"3. I：E"]
[null,"4.氧浓度："]
[null,"5.是否手动通气；"]
[null,"6.安全阀开启压力："]
[null,"7.气源："]
[null,"三、标准配置："]
[null,"1.主机","XX台"]
[null,"2.2L氧气瓶","XX个"]
[null,"3.骨架及防尘包","XX个"]
[null,"4.氧气气源进气输气管","XX套"]
[null,"5.1米螺纹管","XX根"]
[null,"6.充气面罩","XX个"]
[null,"7.呼吸阀及活瓣","XX套"]
[null,"8.3L气囊","XX个"]
[null,"四、其他"]
["除\n颤\n监\n护\n仪","（1)手动除颤和自动除颤均为双向波技术，分为同步和非同步两种方式，能量分20档以上，能量范围1-360J，可通过体外电极板进行能量选择。","是/否"]
[null,"(2) 标配手动除颤、心电、呼吸、自动体外除颤（AED功能，无附件）","是/否"]
[null,"(3) 监护时间","≥XXh，电池可支持360J除颤XX次以上。"]
[null,"(4)具备生理报警和技术报警功能，通过声音、灯光等多种方式进行报警。","是/否"]
[null,"(5) 成人、小儿一体化电极板，可选用除颤起搏监护多功能电极片。","是/否"]
[null,"(6) 支持中文操作界面、AED中文语音提示。","是/否"]
[null,"(7) 彩色TFT显示屏","XX寸, 分辨率XX×XX。最多可显示XX通道监护参数波形。"]
[null,"(8) 有高对比度显示界面。","是/否"]
[null,"(9) 具备外接屏幕显示功能。","是/否"]
[null,"(10)具备记录仪，自动打印除颤记录。","是/否"]
[null,"(11)可存储≥24小时连续ECG波形。","可存储≥24小时连续ECG波形。"]
[null,"(12)数据可导出至电脑查看。","是/否"]
[null,"(13)防水及防摔性能"]
[null,"(14)具有大能量自检、按键、屏幕自检功能。","是/否"]
[null,"(15)数据导出：可通过U盘将数据导出到病人综合数据管理系统软件。","是/否"]
[null,"(16)配备血氧饱和度和血压监测。","是/否"]
[null,"（17）其他"]
["心\n电\n图\n机","(1) 导联：12导联同步采集、显示、打印","是/否"]
[null,"(2) 噪声电平："," XX uVp-p"]
[null,"(3) 频率特性：","XX Hz-XX  Hz"]
[null,"(4) 时间常数：","  XX  S"]
[null,"(5) 输入回路电流：","  XXnA"]
[null,"(6) 耐极化电压：","±XX  mV"]
[null,"(7) 共模拟制比："," XX dB"]
[null,"(8) 心率测量范围","为XX～XXbpm,测量精度为±XX1bpm或XX %。"]
[null,"(9) 具有自动、手动、节律三种显示功能，可同屏显示12道心电波形。","是/否"]
[null,"(10) 记录速度："]
[null,"(11) 触摸屏。","XX英寸 "]
[null,"(12) 支持手写中文输入功能.","是/否"]
[null,"(13) 具有智能环境光检测功能，可根据环境光的强度，自动调节屏幕亮度，屏幕亮度10级可调。","是/否"]
[null,"(14) 具有R-R 分析功能。","是/否"]
[null,"(15) 可存储回顾最近10分钟心电波形。","是/否"]
[null,"(16) 存储","可存XX份病例。"]
[null,"(17) 病历搜索功能，支持姓名、ID号模糊搜索。","是/否"]
[null,"(18) 具有导联连接示意图,能准确判定接触不良的电极，提示各个导联脱落的信息。","是/否"]
[null,"(19) 支持外接键盘、鼠标、条码扫描枪。","是/否"]
[null,"(20) 具有待机唤醒功能，定时关机功能。","是/否"]
[null,"可选配连接USB打印机，直接用普通A4纸打印。","是/否"]
[null,"其他"]
["吸\n引\n器","1．极限负压值："," XX MPa（XX mmHg）"]
[null,"2．负压调节范围: ","XX MPa～极限负压值"]
[null,"3．抽气速率：","XXL/min"]
[null,"4．贮液瓶容量：","XX ml"]
[null,"5．电源：","电源电压： XXV；频率：XX Hz。"]
[null,"6．输入功率：","XX VA"]
[null,"7．熔丝管："]
[null,"其它"]
["商务条款"]
[1,"货物销售合同签订后，货物到货时间。"]
[2,"整机（车）原厂保修, 招标时出具原厂保修承诺。"]
[3,"维修服务机构、配件库以及工程技术人员数量及资质，联系方式。"]
[4,"拟供设备的国家医疗器械三证（含软件注册证）。",null,"需提供复印件"]
[5,"能否提供拟供设备的国家检测报告"]
[6,"能提供的整机免费质保期限（年）"]
[7,"该型号设备在重庆市内各大医院采购情况（列出已采购医院）："]
["备注：1.本表填写请自行加行，所有内容必须填齐。2.拟采购                     ，拟购置数量为      套，预算采购限价为     万元/套。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}